Important Note:

1) Connect Sensor with Computer.

2) Install Driver in proper way and paste essl9000 sensor driver in Folder Path "  C:\Windows\System32\drivers  ".

3)  Check Device in the System in following way :
   (a) Go in Foder path "  Control Panel\All Control Panel Items\System  ".
   (b) Click on Device Manager.
   (c) If device is showing then leave it otherwise Update device with driver from Folder Path " C:\Windows\System32\drivers" for eSSL9000 sensor and for ZKSensor automatic.

4)Insall Software.

5) See all fingers templates



